From 95f09beba70a1f326b1dee2b452edf3c0c48375c Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Wed, 30 Sep 2009 20:05:09 +0000
Subject: Implement the Sansa e200v2 manual.  Please let me know about any
 errors/omissions.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@22861 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index f8768c3ceb..102e138d42 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -539,8 +539,8 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   \opt{sansaAMS}
     {
     The player will boot into the original firmware if it is powered
-    by a USB connection. That feature might go away in the future if
-    Rockbox can handle USB transfers.
+    by a USB connection. This feature may be removed in the future when
+    Rockbox is able to handle USB transfers natively.
     }
 
   \opt{mrobe100}
-- 
cgit v1.2.3

