From 96b8e1bb91203a7ee2d208be442ea230fdc226aa Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Sun, 13 May 2007 16:59:48 +0000
Subject: Make ipod installation a little bit clearer. Introduce a subsection
 called 'Starting original firmware' for targets with dualboot. Improve
 uninstallation instructions as suggested by linuxstb. Closes FS#7079 and
 FS#7086

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@13379 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 73 ++++++++++++++++++---------------------
 1 file changed, 34 insertions(+), 39 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 430cf4837b..85f9a96120 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -167,68 +167,63 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
 
 \label{ref:Safeshutdown}On shutdown, Rockbox automatically saves its settings.
 
+\opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD}{%
+  In the unlikely event of a software failure, a hardware power off can be
+  performed by holding down
+  \opt{PLAYER_PAD}{\ButtonStop}%
+  \opt{RECORDER_PAD,ONDIO_PAD}{\ButtonOff}
+  until the \nopt{ondiosp,ondiofm}{\dap{} power light}%
+  \opt{ondiosp,ondiofm}{\daps{} display} goes off.%
+}
+
 \nopt{gigabeat,x5,archos}
   {
+  \subsection{Starting the original firmware}
+  \label{ref:Dualboot}
   \opt{ipod}
-    {  
-    Rockbox has a dual-boot feature.  To boot into the original firmware, shut 
-    down the device as described above.  Turn on the ``hold'' switch 
-    immediately after turning the player on. Once Rockbox displays the 
-    message ``Loading original firmware ...'' you may turn the ``hold'' 
-    switch off.  Rockbox will boot into the original firmware. 
+    {
+    Rockbox has a dual-boot feature. To boot into the original firmware, shut
+    down the device as described above. Turn on the ``hold'' switch
+    immediately after turning the player on. Once Rockbox displays the
+    message ``Loading original firmware ...'' you may turn the ``hold''
+    switch off. Rockbox will boot into the original firmware.
     
-    \note{The described method of dual-booting works with Rockbox bootloader 
-    version 2, which was released 16 December 2006.  If you have the older 
-    bootloader, boot the original firmware by pressing \ButtonMenu{} 
-    immediately after turning on your Ipod.  Do not release the 
-    \ButtonMenu{} button until you see the ``Loading original firmware...'' 
-    message on the screen.} 
+    \note{The described method of dual-booting works with Rockbox bootloader
+    version 2, which was released 16 December 2006. If you have the older
+    bootloader, boot the original firmware by pressing \ButtonMenu{}
+    immediately after turning on your Ipod.  Do not release the
+    \ButtonMenu{} button until you see the ``Loading original firmware...''
+    message on the screen.}
     
-    Regardless of which method you use to boot to the original firmware, you can 
-    return to Rockbox by pressing and holding \ButtonMenu{} and \ButtonSelect{} 
+    Regardless of which method you use to boot to the original firmware, you can
+    return to Rockbox by pressing and holding \ButtonMenu{} and \ButtonSelect{}
     simultaneously until the player reboots.
     }
 
-  \opt{h1xx}
+  \opt{h1xx,h300}
     {
-    Rockbox has a dual-boot feature.  To boot into the original firmware, 
-    press and hold the \ButtonRec{} button, and then press the \ButtonOn{} 
-    button.
-    }
-  
-  \opt{h300} 
-    { 
-    Rockbox has a dual-boot feature.  To boot into the original firmware, 
-    press and hold the \ButtonRec{} button, and then press and hold the 
-    \ButtonOn{} button.
+    Rockbox has a dual-boot feature. To boot into the original firmware,
+    when the \dap{} is turned off, press and hold the \ButtonRec{} button,
+    and then press the \ButtonOn{} button.
     }
-  
+
   \opt{h10,h10_5gb}
     {
-    Rockbox has a dual-boot feature.  To boot into the original firmware, 
+    Rockbox has a dual-boot feature. To boot into the original firmware,
     press and hold the \ButtonRew{} button while turning on the player.
-    \note{The iriver firmware doesn't shut down properly when you turn it off, 
-    it only goes to sleep. To get back into Rockbox when exiting from the 
+    \note{The iriver firmware doesn't shut down properly when you turn it off,
+    it only goes to sleep. To get back into Rockbox when exiting from the
     iriver firmware, you will need to reset the player by \opt{h10}{inserting a
     pin in the reset hole}\opt{h10_5gb}{taking out battery}.}
     }
     
   \opt{e200}
     {
-    Rockbox has a dual-boot feature.  To boot into the original firmware, 
+    Rockbox has a dual-boot feature. To boot into the original firmware,
     press and hold the \ButtonLeft{} button while turning on the player.
     }
   }
 
-
-\opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD}{%
-  In the unlikely event of a software failure, a hardware power off can be
-  performed by holding down
-  \opt{PLAYER_PAD}{\ButtonStop}%
-  \opt{RECORDER_PAD,ONDIO_PAD}{\ButtonOff}
-  until the \nopt{ondiosp,ondiofm}{\dap{} power light}%
-  \opt{ondiosp,ondiofm}{\daps{} display} goes off.%
-}
 \subsection{The first contact}
 
 After you have first started the \dap{} you'll be presented by the
-- 
cgit v1.2.3

