From a05e5cc1337755e50efc8a51d626adcbd9189306 Mon Sep 17 00:00:00 2001
From: Christi Scarborough <christi@coraline.org>
Date: Sat, 19 May 2007 19:54:33 +0000
Subject: Physical description for the Cowon Iaudio X5/M5.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@13425 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 25 ++++++++++++++++++++++++-
 1 file changed, 24 insertions(+), 1 deletion(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 94351bd21b..f6f23eb9eb 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -164,7 +164,30 @@ paragraph.
   button and nearest to the top of the unit the \ButtonPower{} button, which is held
   down to turn the \dap{} on or off.}
   %
-  \nopt{h1xx,h300,ipodnano,ipodvideo,ipodmini,ipod4g,ipod3g,ipodcolor,ondio,h10,h10_5gb,gigabeatf}
+  \opt{x5,m5}{
+  The \dap{} is curved so that the end with the screen on it is thicker than the 
+  other end.  Hold the \dap{} wih the thick end towards the top and the screen
+  facing towards you.  Half way up the front of the unit on the right hand side
+  is a four way joystick which is the \ButtonUp{}, \ButtonDown{}, 
+  \ButtonLeft{}, and \ButtonRight{} buttons.  
+  
+  On the right hand side of the \dap{} from top to bottom, first there is a two 
+  way switch.  the \ButtonPower{} button is activated by pushing this switch up,
+  and pusing this swtich down until it clicks slightly will activate the 
+  \ButtonHold{} button.  When the switch is in this position, none of the other
+  keys will have an effect.
+  
+  Below the switch is a lozenge shaped button which is the \ButtonRecord{} 
+  button, and below that the final button on this side of the unit, the 
+  \ButoonPlay{} button.  On the bottom of the unit is the connecter for the 
+  \playerman{} subpack or dock.  On the top of the unit is a charge 
+  indicator light, which may feel a bit like a button, but isn't.
+  
+  From the top of the \dap{} on the left hand side is the headphone socket, then the 
+  remote connector.  Below this is a cover which protects the \opt{x5}{USB host
+  connector.}\opt{m5}{USB and charging connector}.}
+  %
+  \nopt{h1xx,h300,ipodnano,ipodvideo,ipodmini,ipod4g,ipod3g,ipodcolor,ondio,h10,h10_5gb,gigabeatf,x5,m5}
   {
     \fixme{Write a section describing the \dap{} for blind users.}
   }
-- 
cgit v1.2.3

