From a969bc0d23b923d0c83a5eafed7d9212a2b3a1c4 Mon Sep 17 00:00:00 2001
From: Marc Guay <marcguay@rockbox.org>
Date: Sun, 29 Jun 2008 17:38:27 +0000
Subject: Manual: Add keymaps for all targets to the 'hardware power off' piece
 in the Quick Start chapter.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@17880 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 18 +++++++++++-------
 1 file changed, 11 insertions(+), 7 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 8d1ef8940f..1ec2565cba 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -352,13 +352,17 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   the Reset Settings in \reference{ref:manage_settings_menu} for details.
 }%
 
-\opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD}{%
-  In the unlikely event of a software failure, a hardware power off can be
-  performed by holding down
-  \opt{PLAYER_PAD}{\ButtonStop}%
-  \opt{RECORDER_PAD,ONDIO_PAD}{\ButtonOff}
-  until the \nopt{ondiosp,ondiofm}{\dap{} power light}%
-  \opt{ondiosp,ondiofm}{\daps{} display} goes off.%
+In the unlikely event of a software failure, a hardware power off can be
+performed by
+\opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD,GIGABEAT_PAD,IPOD_4G_PAD,SANSA_E200_PAD%
+,SANSA_C200_PAD,IAUDIO_X5_PAD,IAUDIO_M5_PAD}{%
+  holding down \opt{PLAYER_PAD}{\ButtonStop}\opt{RECORDER_PAD,ONDIO_PAD}
+  {\ButtonOff}\opt{GIGABEAT_PAD}{the battery switch}\opt{IPOD_4G_PAD}
+  {\ButtonMenu + \ButtonSelect}\opt{SANSA_E200_PAD,SANSA_C200_PAD,IAUDIO_X5_PAD%
+  ,IAUDIO_M5_PAD}{\ButtonPower} until the \dap{} shuts off.
+}%
+\opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_M3_PAD}{%
+  inserting a paperclip gently into the Reset hole.
 }%
 
 \nopt{gigabeatf,m5,x5,archos}
-- 
cgit v1.2.3

