From b02123d349cb7ec914633b4233d6838dfe5a9b46 Mon Sep 17 00:00:00 2001
From: Dana Conrad <dconrad@fastmail.com>
Date: Tue, 5 Apr 2022 21:59:37 -0500
Subject: Manual: Add Eros Q Native

Here is the PDF this patchset produces: https://www.dropbox.com/s/v1uz8p2fsgsz1ng/rockbox-erosqnative-923dabb5cd-220409.pdf?dl=0

Change-Id: I27554cb65a6498a6ccb714d4f93f25264b516e99
---
 manual/rockbox_interface/main.tex | 14 ++++++++------
 1 file changed, 8 insertions(+), 6 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index ccc6e25ae6..20aa8c833e 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -518,7 +518,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{IPOD_3G_PAD}{\ButtonMenu{} / \ButtonPlay}%
       \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,ONDA_VX777_PAD%
           ,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS,PBELL_VIBE500_PAD%
-          ,SANSA_FUZEPLUS_PAD,XDUOO_X3_PAD%
+          ,SANSA_FUZEPLUS_PAD,XDUOO_X3_PAD,AIGO_EROSQ_PAD%
           }{\ButtonPower}%
       \opt{COWON_D2_PAD} {\ButtonPower{}, then \ButtonHold}%
       \opt{ONDA_VX777_PAD} {\ButtonPower{}}%
@@ -538,7 +538,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{IPOD_4G_PAD,IPOD_3G_PAD}{Long \ButtonPlay}%
       \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD%
           ,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS,COWON_D2_PAD%
-          ,PBELL_VIBE500_PAD,ONDA_VX777_PAD,SANSA_FUZEPLUS_PAD,XDUOO_X3_PAD%
+          ,PBELL_VIBE500_PAD,ONDA_VX777_PAD,SANSA_FUZEPLUS_PAD,XDUOO_X3_PAD,AIGO_EROSQ_PAD%
           }{Long \ButtonPower}%
       \opt{AGPTEK_ROCKER_PAD}{Long \ButtonPower{}}%
           &
@@ -721,15 +721,17 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     and then press the \ButtonPower{} button.
     }
 
-  \opt{fiiom3k,shanlingq1}
+  \opt{fiiom3k,shanlingq1,erosqnative}
     {
     Rockbox has a dual-boot feature. To boot into the original firmware,
     hold \ActionBootOFPlayer{} when powering on the \dap{}.
 
-    You can trigger a normal \playerman{} firmware update by holding
-    \ActionBootOFRecovery{} when powering on the \dap{}.
-    \warn{Updating the original firmware will \textbf{erase} the Rockbox
+    \nopt{erosqnative}{
+      You can trigger a normal \playerman{} firmware update by holding
+      \ActionBootOFRecovery{} when powering on the \dap{}.
+      \warn{Updating the original firmware will \textbf{erase} the Rockbox
       bootloader.}
+    }
 
     \subsection{Entering the recovery menu}
     You can access the Rockbox bootloader's ``recovery menu'' by holding
-- 
cgit v1.2.3

