From bf83ac624083af0c53fdc358df8270798831d8cb Mon Sep 17 00:00:00 2001
From: Marianne Arnold <pixelma@rockbox.org>
Date: Sun, 4 Jul 2010 13:28:20 +0000
Subject: Add platform and keymap files and basic descriptions about installing
 Rockbox etc. for an Onda VX777 manual. Author: Giovanni Zilli. Flyspray:
 FS#11437.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@27279 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 33 +++++++++++++++++++--------------
 1 file changed, 19 insertions(+), 14 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 507255bcf3..8a69744f17 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -22,18 +22,16 @@ picture above.
 \opt{touchscreen}{
 The areas of the touchscreen in the 3$\times$3 grid mode are in turn referred as follows:
 \begin{table}
-    \begin{center}
-    %\begin{tabularx}{.82\textwidth}{l|c|r}
-    \begin{tabularx}{.9\textwidth}{X|X|X}
-    \toprule
-        \TouchTopLeft & \TouchTopMiddle & \TouchTopRight \\
-    \midrule
-        \TouchMidLeft & \TouchCenter & \TouchMidRight \\
-    \midrule
-        \TouchBottomLeft & \TouchBottomMiddle & \TouchBottomRight \\
-    \bottomrule
-    \end{tabularx}
-    \end{center}
+    \centering
+    \begin{tabular}{|c|c|c|}
+	\hline
+        \TouchTopLeft & \TouchTopMiddle & \TouchTopRight \\ [5ex]
+	\hline        
+	\TouchMidLeft & \TouchCenter & \TouchMidRight \\ [5ex]
+	\hline        
+	\TouchBottomLeft & \TouchBottomMiddle & \TouchBottomRight \\ [5ex]
+	\hline
+    \end{tabular}
 \end{table}
 }%
 Whenever a button name is prefixed by ``Long'', a long press of approximately
@@ -503,7 +501,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{IPOD_3G_PAD}{\ButtonMenu{} / \ButtonPlay}%
       \opt{ONDIO_PAD}{\ButtonOff}\opt{RECORDER_PAD,PLAYER_PAD}%
           {Long \ButtonOn}%
-      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD%
+      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,ONDA_VX777_PAD%
           ,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS,PBELL_VIBE500_PAD%
           }{\ButtonPower}%
       \opt{COWON_D2_PAD} {\ButtonPower{}, then \ButtonHold}%
@@ -522,7 +520,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{PLAYER_PAD}{From the Main Menu, select \textbf{Shutdown}}%
       \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD%
           ,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS,COWON_D2_PAD%
-          ,PBELL_VIBE500_PAD}{Long \ButtonPower}%
+          ,PBELL_VIBE500_PAD,ONDA_VX777_PAD}{Long \ButtonPower}%
           &
       \opt{HAVEREMOTEKEYMAP}{ 
           \opt{IRIVER_RC_H100_PAD}{Long \ButtonRCStop}%
@@ -657,6 +655,13 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     button and keep it pressed until the original firmware starts.
     }
 
+  \opt{ondavx777}
+    {
+    Rockbox has a dual-boot feature where it is possible to load the original firmware from
+    the file \fname{/SD/ccpmp.bin}. To boot into the original firmware press and release
+    \ButtonPower{} immediately after the Rockbox Logo appear on the screen.
+    }
+
   }
 \subsection{Putting music on your \dap{}}
 
-- 
cgit v1.2.3

