From c1e86f7531e82936cc5c33fce5b7231787cfd84a Mon Sep 17 00:00:00 2001
From: Frank Gevaerts <frank@gevaerts.be>
Date: Fri, 5 Sep 2008 18:55:38 +0000
Subject: Adds descriptions to the manual for the iPod 1st, 2nd, and 3rd
 generations, and fixes some problems with the nano and Sansa c200 manuals
 (FS#9367 by Robert Menes)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@18423 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 67 +++++++++++++++++++++++++++++++++++----
 1 file changed, 60 insertions(+), 7 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 50057e0854..58957151b0 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -60,15 +60,14 @@ described in detail in the following paragraph.
   used in Rockbox. 
   }
   %
-  \opt{ipod4g,ipod3g,ipodcolor,ipodvideo,ipodmini}
-  { 
+  \opt{ipod4g,ipodcolor,ipodvideo,ipodmini}{ 
   The main controls on the \dap{} are a slightly indented scroll wheel 
   with a flat round button in the center. Hold the \dap{} with these controls 
   facing you. 
 
   The top of the player will have the following, from left to 
   right:
-  \opt{ipod4g, ipod3g ,ipodcolor}{remote connector, headphone jack, \ButtonHold{} 
+  \opt{ipod4g,ipodcolor}{remote connector, headphone jack, \ButtonHold{} 
     switch.}
   \opt{ipodvideo}{\ButtonHold{} switch, headphone jack.}
   \opt{ipodmini}{\ButtonHold{} switch, remote connector, headphone jack.}	
@@ -85,6 +84,59 @@ described in detail in the following paragraph.
   counterclockwise. Note that the wheel is sensitive, so you will need to move
   slowly at first and get a feel for how it works.
   
+  Note that when the \ButtonHold{} switch is pushed toward the center of the \dap{}, 
+  hold is on, and none of the other controls do anything.  Be sure
+  \ButtonHold{} is off before trying to use your player. 
+  }
+  %
+  \opt{ipod3g}{ 
+  The main controls on the \dap{} are a slightly indented touch wheel 
+  with a flat round button in the center, and four buttons in a row above the
+  touch wheel. Hold the \dap{} with these controls 
+  facing you. 
+
+  The top of the player will have the following, from left to 
+  right: remote connector, headphone jack, \ButtonHold{} switch.
+	
+  The dock connector that is used to connect your \dap{} to your computer is on 
+  the bottom panel of the \dap{}.
+
+  The button in the middle of the wheel is called \ButtonSelect{}. You can
+  operate the wheel by sliding your finger around it.  The row of
+  buttons consists of, from left to right, the \ButtonLeft{},
+  \ButtonMenu{}, \ButtonPlay{}, and \ButtonRight{} buttons.
+  When the manual says to \ButtonScrollFwd{}, it means to slide your finger
+  clockwise around the wheel. \ButtonScrollBack{} means to slide your finger
+  counterclockwise. Note that the wheel is sensitive, so you will need to move
+  slowly at first and get a feel for how it works.
+  
+  Note that when the \ButtonHold{} switch is pushed toward the center of the \dap{}, 
+  hold is on, and none of the other controls do anything.  Be sure
+  \ButtonHold{} is off before trying to use your player. 
+  }
+  %
+  \opt{ipod1g2g}{ 
+  The main controls on the \dap{} are a slightly indented wheel 
+  with a flat round button in the center, and four buttons surrounding
+  it. On the 1st generation iPod, this wheel physically turns. On the
+  2nd generation iPod, this wheel is touch-sensitive. Hold the \dap{} with these controls 
+  facing you. 
+
+  The top of the player will have the following, from left to 
+  right: FireWire port, headphone jack, \ButtonHold{} switch.
+
+  The FireWire port is used to connect your \dap{} to the computer and
+  to charge its battery via a wall charger.
+	
+  The button in the middle of the wheel is called \ButtonSelect{}. You can
+  operate the wheel by turning it, or sliding your finger around
+  it. The top is \ButtonMenu{}, the bottom is \ButtonPlay{}, the left
+  is \ButtonLeft{}, and the right is \ButtonRight{}.
+  When the manual says to \ButtonScrollFwd{}, it means to slide your finger
+  clockwise around the wheel. \ButtonScrollBack{} means to slide your finger
+  counterclockwise. Note that the wheel is sensitive, so you will need to move
+  slowly at first and get a feel for how it works.
+  
   Note that when the \ButtonHold{} switch is pushed toward the center of the \dap{}, 
   hold is on, and none of the other controls do anything.  Be sure
   \ButtonHold{} is off before trying to use your player. 
@@ -93,13 +145,14 @@ described in detail in the following paragraph.
   \opt{ipodnano}{
   The main controls on the \dap{} are a slightly indented wheel with a
   flat round button in the center. Hold the \dap{} with these controls on the
-  top surface. There is a \ButtonHold{} switch at one end, and headphone and USB
-  jacks at the other; be sure the end with the switch is facing away from you.
+  top surface. There is a \ButtonHold{} switch at one end, and
+  headphone and dock connector at the other; be sure the end with the
+  switch is facing away from you.
 
   The button in the middle of the wheel is called \ButtonSelect{}. You can
   operate the wheel by pressing the top, bottom, left or right sections,
   or by sliding your finger around it.  The top is \ButtonMenu{}, the bottom is
-  \ButtonPlay, the left is \ButtonLeft, and the right is \ButtonRight{}.
+  \ButtonPlay{}, the left is \ButtonLeft{}, and the right is \ButtonRight{}.
   When the manual says to \ButtonScrollFwd{}, it means to slide your finger
   clockwise around the wheel. \ButtonScrollBack{} means to slide your finger
   counterclockwise. Note that the wheel is sensitive, so you will need to move
@@ -266,7 +319,7 @@ described in detail in the following paragraph.
   raised triangle on the \ButtonVolUp{} button. To the right of
   the volume buttons on the top of the unit is the slot for inserting flash
   memory cards. On the right side of the unit is the connector for the USB
-  cable. At center of the bottom of the dap{} is the \ButtonRec{} button. To
+  cable. At center of the bottom of the \dap{} is the \ButtonRec{} button. To
   the left of the \ButtonRec{} button is the \ButtonHold{} switch. Moving this
   switch to the right activates hold mode, in which none of the other buttons
   have any effect. On the lower left side of the unit is the headphone socket.
-- 
cgit v1.2.3

