From c5bffb1289ea0f2042d1b6523b29b46a41368bb5 Mon Sep 17 00:00:00 2001
From: Robert Menes <rmenes@rockbox.org>
Date: Thu, 29 Jan 2009 04:11:44 +0000
Subject: Some various pieces of manual work: Fixed installation instructions
 for the e200 and c200 under Mac OS X, added a warning about v2 firmwares to
 the Sansa install page, and the very beginnings of a Sansa Clip manual (which
 still needs a lot of work!) Also fixed up the blind descriptions for the
 Archos Player and Recorder, and some little typo fixes here and there.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19878 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 65 +++++++++++++++++++++++++++------------
 1 file changed, 46 insertions(+), 19 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index f99235b574..eb2599ddda 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -173,20 +173,21 @@ described in detail in the following paragraph.
   }
   %
   \opt{ondio}{
-  The main characteristic of the Ondio case is the dent on its lower right side
+  The main characteristic of the Ondio case is the indent on its lower right side, 
   which is the MMC slot. Holding the \dap{} with this slot in the described position
   you'll find the following:
 
-  On the curved top it has the headphone jack to the left,
-  the \ButtonOff{} button is in the middle%
-  \opt{recording}{ and the line in jack to the right}.
-  Apart from the already mentioned MMC slot you will find the USB connector on
-  the \daps{} right side. Placed on the upper side of the device right below
-  the flat display there is the main button pad of the \dap{}. A strong deepening
-  marks the center of it and helps to operate the directional keys from there.
-  \ButtonLeft{} and \ButtonRight{} form some sort of a strip and divide \ButtonUp{}
-  and \ButtonDown{}. The raised button positioned in the lower left of this round
-  crosspad is labelled \ButtonMenu{}.}
+  On the curved top, from left to right, are the headphone jack,
+  the \ButtonOff{} button,%
+  \opt{recording}{ and the line in jack}.
+  Apart from the already mentioned MMC slot, you will find the USB connector on
+  the \daps{} right side. Below the LCD, at approximately the center of the \dap{},
+  there is the main button pad of the \dap{}. The centre of the button pad dips inward
+  and helps to operate the directional keys from there. Located on a two-way button
+  strip are the \ButtonLeft{} and \ButtonRight{} keys, with \ButtonUp{} above it
+  and \ButtonDown{} below it. The raised button positioned in the lower left of this 
+  round crosspad is labelled \ButtonMenu{}.
+  }
   %
   \opt{h10,h10_5gb}{
   Hold or lay the \dap{} so that the side with the scroll pad and
@@ -284,7 +285,7 @@ described in detail in the following paragraph.
   other end.  Hold the \dap{} wih the thick end towards the top and the screen
   facing towards you.  Half way up the front of the unit on the right hand side
   is a four way joystick which is the \ButtonUp{}, \ButtonDown{}, 
-  \ButtonLeft{}, and \ButtonRight{} buttons. When pressed it serves as \ButtonSelect.
+  \ButtonLeft{}, and \ButtonRight{} buttons. When pressed it serves as \ButtonSelect{}.
   
   On the right hand side of the \dap{} from top to bottom, first there is a two 
   way switch.  the \ButtonPower{} button is activated by pushing this switch up,
@@ -345,15 +346,37 @@ described in detail in the following paragraph.
   Immediately above the headphone socket is a lanyard loop and the microphone.
   }
   %
+  \opt{clip}{
+  Hold the \dap{} with the controls on the bottom and the screen on the top. The main
+  controls are a four-way pad with a button in the centre; pressing this centre button
+  functions as \ButtonSelect{}. Going clockwise from the top, the four-way pad contains
+  the \ButtonUp{}, \ButtonRight{}, \ButtonDown{}, and \ButtonLeft{} buttons. 
+  Immediately above and to the right of the four-way pad is the \ButtonHome{} button.
+
+  On the left hand panel is a two way switch. Pressing this switch up acts as
+  \ButtonPower{}, and clicking it down until it locks acts as the \ButtonHold{}
+  switch. When the \ButtonHold{} switch is on, none of the other buttons have any
+  effect. Immediately above the switch is a mini-USB port to connect the \dap{} to
+  a computer.
+
+  On the right hand panel is a two-way button that acts as \ButtonVolDown{} when
+  pressed on the bottom, and \ButtonVolUp{} when pressed on the top. Immediately
+  above this button is the headphone jack.
+  }
+  %
   \opt{player}{
-  Holding the Jukebox in front of you there should be two buttons to
-  the left of the unit and a single multi-way circular button to their right.
-  The buttons are as follows.%
+  The main controls of this player are a four-way button on the right below
+  the screen, and two round buttons to the left of it. Hold the \dap{} with
+  these controls on the bottom and facing you.
+
   On the left hand side, the higher of the two small buttons is the \ButtonOn{},
   the lower of the two buttons is the \ButtonMenu{} button. The large circular
-  button on the right - push towards the top serves as \ButtonPlay{}, push towards
-  the left is called \ButtonLeft{}, push towards the right \ButtonRight{} and push
-  towards the bottom is labelled \ButtonStop{}.
+  button on the right contains, clockwise from the top, the \ButtonPlay{},
+  the \ButtonRight{}, the \ButtonStop{}, and the \ButtonLeft{} buttons.
+
+  On the top on the \dap{} is the headphone jack on the left and the Line-Out
+  jack on the right. On the bottom of the \dap{} is the Line-In jack on the left,
+  the DC-In jack on the right, and the USB connector in the centre.
   }
   %
   \opt{recorder}{
@@ -372,6 +395,10 @@ described in detail in the following paragraph.
   below the \ButtonPlay{} button there is the \ButtonDown{} button placed. In the row
   of three rectangular buttons the following buttons can be found (from left to right):
   \ButtonFOne{}, \ButtonFTwo{} and \ButtonFThree{}.
+
+  On the top of the \dap{} is the headphone jack on the left and the Line-Out jack on
+  the right. On the bottom of the \dap{} is the Line-In jack on the left, the
+  DC-In jack on the right, and the USB connector in the centre.
   }
   \opt{recorderv2fm}{
   Holding the Jukebox in front of you, there should be three rectangular buttons
@@ -489,7 +516,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     \note{The iriver firmware does not shut down properly when you turn it off,
     it only goes to sleep. To get back into Rockbox when exiting from the
     iriver firmware, you will need to reset the player by \opt{h10}{inserting a
-    pin in the reset hole}\opt{h10_5gb}{taking out battery}.}
+    pin in the reset hole}\opt{h10_5gb}{removing and reinserting the battery}.}
     }
     
   \opt{sansa}
-- 
cgit v1.2.3

