From cb435ab5c1ffc5ab0ad2c14f41cb67bf4d8b6a66 Mon Sep 17 00:00:00 2001
From: Rafaël Carré <rafael.carre@gmail.com>
Date: Mon, 6 Sep 2010 05:24:16 +0000
Subject: manual: the AMSv1 don't run OF if powered by USB

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@28002 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 8303b647ef..195b04e1c0 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -615,7 +615,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     press and hold the \ButtonLeft{} button while turning on the player.
     }
 
-  \opt{sansaAMS}
+  \opt{clipv2,fuzev2,clipplus}
     {
     The player will always boot into the original firmware if it is powered
     by a USB connection, and additionally will do so if USB is inserted while
-- 
cgit v1.2.3

