From e3c9d6a3590fadf73250535bac94817501eac30a Mon Sep 17 00:00:00 2001
From: Rafaël Carré <rafael.carre@gmail.com>
Date: Fri, 22 May 2009 10:44:15 +0000
Subject: Initial work on the Fuze manual

Still missing:
    - svg/pdf/nice png front image
    - plugin keymaps
    - manual install instructions for sansav2 (and mkamsboot binaries)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@21031 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 13 ++++++++++---
 1 file changed, 10 insertions(+), 3 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 48b471cd98..43851489a1 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -428,7 +428,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{IPOD_3G_PAD}{\ButtonMenu{} / \ButtonPlay}%
       \opt{ONDIO_PAD}{\ButtonOff}\opt{RECORDER_PAD,PLAYER_PAD}%
           {Long \ButtonOn}%
-      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD}
+      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS}
           {\ButtonPower}%
       & Start Rockbox\\
       \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{Long \ButtonOff}%
@@ -436,7 +436,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
       \opt{ONDIO_PAD,recorderv2fm}{Long \ButtonOff}%
       \opt{recorder}{Double tap \ButtonOff\ when playback is stopped}%
       \opt{PLAYER_PAD}{From the Main Menu, select \textbf{Shutdown}}%
-      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD}%
+      \opt{IAUDIO_X5_PAD,IRIVER_H10_PAD,SANSA_E200_PAD,SANSA_C200_PAD,GIGABEAT_PAD,MROBE100_PAD,GIGABEAT_S_PAD,sansaAMS}%
           {Long \ButtonPower}%
       & Shutdown Rockbox\\
     \end{btnmap}
@@ -519,12 +519,19 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     pin in the reset hole}\opt{h10_5gb}{removing and reinserting the battery}.}
     }
     
-  \opt{sansa}
+  \opt{sansa,sansaAMS}
     {
     Rockbox has a dual-boot feature. To boot into the original firmware,
     press and hold the \ButtonLeft{} button while turning on the player.
     }
 
+  \opt{sansaAMS}
+    {
+    The player will boot into the original firmware if it is powered
+    by a USB connection. That feature might go away in the future if
+    Rockbox can handle USB transfers.
+    }
+
   \opt{mrobe100}
     {
     Rockbox has a dual-boot feature. It loads the original firmware from
-- 
cgit v1.2.3

