From e66a780350a7aa6ea0ad0c272ab1fb57d6d87105 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Sun, 28 Feb 2010 12:22:08 +0000
Subject: Correct reset and disk mode combinations for 1G - 3G iPods.  Closes
 FS#11011.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@24966 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 0cf077d3c4..7769ac8e29 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -513,7 +513,8 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   In the unlikely event of a software failure, hardware poweroff or reset can be
   performed by holding down \opt{PLAYER_PAD}{\ButtonStop}\opt{RECORDER_PAD,ONDIO_PAD}
   {\ButtonOff}\opt{GIGABEAT_PAD}{the battery switch}\opt{IPOD_4G_PAD}
-  {\ButtonMenu + \ButtonSelect}\opt{IPOD_3G_PAD}{\ButtonMenu + \ButtonPlay}
+  {\ButtonMenu{} and \ButtonSelect{} simultaneously}%
+  \opt{IPOD_3G_PAD}{\ButtonMenu{} and \ButtonPlay{} simultaneously}%
   \opt{SANSA_E200_PAD,SANSA_C200_PAD,IAUDIO_X5_PAD,IAUDIO_M5_PAD}
   {\ButtonPower} until the \dap{} shuts off or reboots.
 }%
-- 
cgit v1.2.3

