From efc756a9fc0ccdb835300351c78c28c1dd501118 Mon Sep 17 00:00:00 2001
From: Michael Giacomelli <giac2000@hotmail.com>
Date: Fri, 15 Jan 2010 21:30:58 +0000
Subject: Clarify boot to OF on USB insert for Sansa AMS to make clear that the
 player will always boot to the OF on USB power up.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@24241 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 8 +++++---
 1 file changed, 5 insertions(+), 3 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 398766d5b9..77ca9cdbed 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -584,9 +584,11 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
 
   \opt{sansaAMS}
     {
-    The player will boot into the original firmware if it is powered
-    by a USB connection. This feature may be removed in the future when
-    Rockbox is able to handle USB transfers natively.
+    The player will always boot into the original firmware if it is powered
+    by a USB connection, and additionally will do so if USB is inserted while
+	rockbox is running without holding \ActionStdUsbCharge{}. This feature may
+	be removed in the future when Rockbox is able to handle USB transfers 
+	natively.
     }
 
   \opt{mrobe100}
-- 
cgit v1.2.3

