From f498d53d72007124049cf72ccccf3435abb097fe Mon Sep 17 00:00:00 2001
From: Dominik Riebeling <Dominik.Riebeling@gmail.com>
Date: Sun, 7 Dec 2008 23:00:15 +0000
Subject: Rename h100 manual name "h1xx" to "h100" to be in line with other
 players.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19361 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 93fea71d1b..a0ad76cf54 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -22,7 +22,7 @@ described in detail in the following paragraph.
   \wikilink{BlindFAQ}.
   
   %
-  \opt{h1xx}{ 
+  \opt{h100}{ 
   If you put the \dap{} on a table with the joystick pointing 
   towards you, and the curved sides at the top, you will find the following 
   if you start from the top-right corner and follow the side of the \dap{} in a
@@ -455,7 +455,7 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
     simultaneously until the player hard resets.
     }
 
-  \opt{h1xx,h300}
+  \opt{h100,h300}
     {
     Rockbox has a dual-boot feature. To boot into the original firmware,
     when the \dap{} is turned off, press and hold the \ButtonRec{} button,
-- 
cgit v1.2.3

