From fadc439259a239c2f5b55e2bd00f45a9b059bc68 Mon Sep 17 00:00:00 2001
From: Marc Guay <marcguay@rockbox.org>
Date: Sun, 29 Jun 2008 18:36:34 +0000
Subject: Make sure the iPods don't have a hanging sentence in my last manual
 addition.  They don't have a hardware power off so keep the line inside the
 \opts.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@17882 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 1ec2565cba..0fd013ef15 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -352,17 +352,17 @@ To turn on and off your Rockbox enabled \dap{} use the following keys:
   the Reset Settings in \reference{ref:manage_settings_menu} for details.
 }%
 
-In the unlikely event of a software failure, a hardware power off can be
-performed by
 \opt{PLAYER_PAD,RECORDER_PAD,ONDIO_PAD,GIGABEAT_PAD,IPOD_4G_PAD,SANSA_E200_PAD%
 ,SANSA_C200_PAD,IAUDIO_X5_PAD,IAUDIO_M5_PAD}{%
-  holding down \opt{PLAYER_PAD}{\ButtonStop}\opt{RECORDER_PAD,ONDIO_PAD}
+  In the unlikely event of a software failure, a hardware power off can be
+  performed by holding down \opt{PLAYER_PAD}{\ButtonStop}\opt{RECORDER_PAD,ONDIO_PAD}
   {\ButtonOff}\opt{GIGABEAT_PAD}{the battery switch}\opt{IPOD_4G_PAD}
   {\ButtonMenu + \ButtonSelect}\opt{SANSA_E200_PAD,SANSA_C200_PAD,IAUDIO_X5_PAD%
   ,IAUDIO_M5_PAD}{\ButtonPower} until the \dap{} shuts off.
 }%
 \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_M3_PAD}{%
-  inserting a paperclip gently into the Reset hole.
+  In the unlikely event of a software failure, a hardware power off can be
+  performed by inserting a paperclip gently into the Reset hole.
 }%
 
 \nopt{gigabeatf,m5,x5,archos}
-- 
cgit v1.2.3

