From fb07e4410442347e9c2623e2002c8faeac93d3c6 Mon Sep 17 00:00:00 2001
From: Marianne Arnold <pixelma@rockbox.org>
Date: Sat, 19 May 2007 21:24:52 +0000
Subject: Fix some typos to make the three affected manuals build again

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@13432 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 16 ++++++++--------
 1 file changed, 8 insertions(+), 8 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index c809fe91a9..670078af5a 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -152,7 +152,7 @@ paragraph.
   top of the unit from left to right are the power socket, the \ButtonHold{} 
   switch, and the headphone socket.  The \ButtonHold{} switch puts the \dap{} into
   hold mode when it is switched to the right 
-  of the unit.  THe buttons will have no effect when this is the case.  
+  of the unit. The buttons will have no effect when this is the case.  
   
   Starting from the left hand side on the bottom of the unit, nearer to the front
   than the back, is a recessed switch which 
@@ -164,7 +164,7 @@ paragraph.
   
   Finally on the right hand side of the unit are some control buttons.  Going from
   the bottom of the unit to the top there is a small round \ButtonA{} buttton then a
-  rocker volume switch with of the \ButttonVolDown{} button below the \ButtonVolUp{}
+  rocker volume switch with of the \ButtonVolDown{} button below the \ButtonVolUp{}
   button.  Above that is are two more small round buttons, the \ButtonMenu{} 
   button and nearest to the top of the unit the \ButtonPower{} button, which is held
   down to turn the \dap{} on or off.}
@@ -174,17 +174,17 @@ paragraph.
   other end.  Hold the \dap{} wih the thick end towards the top and the screen
   facing towards you.  Half way up the front of the unit on the right hand side
   is a four way joystick which is the \ButtonUp{}, \ButtonDown{}, 
-  \ButtonLeft{}, and \ButtonRight{} buttons.  
+  \ButtonLeft{}, and \ButtonRight{} buttons. When pressed it serves as \ButtonSelect.
   
   On the right hand side of the \dap{} from top to bottom, first there is a two 
   way switch.  the \ButtonPower{} button is activated by pushing this switch up,
-  and pusing this swtich down until it clicks slightly will activate the 
+  and pusing this switch down until it clicks slightly will activate the 
   \ButtonHold{} button.  When the switch is in this position, none of the other
   keys will have an effect.
   
-  Below the switch is a lozenge shaped button which is the \ButtonRecord{} 
+  Below the switch is a lozenge shaped button which is the \ButtonRec{} 
   button, and below that the final button on this side of the unit, the 
-  \ButoonPlay{} button.  Just below this is a small hole which is difficult to
+  \ButtonPlay{} button.  Just below this is a small hole which is difficult to
   locate by touch which is the internal microphone.  At the very bottom of 
   this side of the unit is the reset hole, which can be used to perform a hard
   reset by inserting a paper clip.
@@ -198,7 +198,7 @@ paragraph.
   connector.}\opt{m5}{USB and charging connector}.}
   %
   \opt{e200}{
-  Hold the \dap with the turning wheel at the front and bottom.  On the bottom left
+  Hold the \dap{} with the turning wheel at the front and bottom.  On the bottom left
   of the front of the \dap{} is a raised round button, the \ButtonPower{} button.
   Above and to the left of this, on the outside of the turning wheel are four 
   buttons.  These are the \ButtonUp{}, \ButtonDown{}, \ButtonLeft{} and 
@@ -207,7 +207,7 @@ paragraph.
   left, the \ButtonScrollUp{} function.  
   
   On the right of the unit is a slot for inserting flash cards.  On the bottom is 
-  the connector for the USB cable.  On the left is the \ButtonRecord{} button, and
+  the connector for the USB cable.  On the left is the \ButtonRec{} button, and
   on the top, there is the headphone socket to the right, and the \ButtonHold{}
   switch.  Moving this switch to the right activates hold mode in which none of the
   other buttons have any effect.  Just to the left of the \ButtonHold{} switch is a
-- 
cgit v1.2.3

