From 1248e9c6de7687ee7bb76e43dcebac2e0575ecc7 Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Wed, 14 Apr 2010 20:38:21 +0000
Subject: More work on consistent usage of units in the manual. Use
 non-breaking spaces if applicable.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25649 a1c6a512-1295-4272-9138-f99709370657
---
 manual/appendix/appendix.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/appendix/appendix.tex')

diff --git a/manual/appendix/appendix.tex b/manual/appendix/appendix.tex
index 99bc626cfa..fe0ffe97e8 100644
--- a/manual/appendix/appendix.tex
+++ b/manual/appendix/appendix.tex
@@ -73,7 +73,7 @@ The recording hardware (the MAS) does not allow us to do this
   The mp3{}-decoding hardware cannot decode OGG. It can be reprogrammed, but 
   there is too little memory for OGG and we have no documentation on how to 
   program the MAS' DSP. Doing the conversion with the CPU is impossible, since 
-  a 12 MHz SH1 is far too slow for this daunting task.
+  a 12~MHz SH1 is far too slow for this daunting task.
 \item Archos Multimedia support.\\
   The Archos Multimedia is a completely different beast. It is an entirely 
   different architecture, different CPU and upgrading the software is done 
-- 
cgit v1.2.3

