From 15f1057cc021f627d8eb2cd453a1e659af1af1fc Mon Sep 17 00:00:00 2001
From: Jonathan Gordon <rockbox@jdgordon.info>
Date: Sat, 9 Feb 2013 23:27:22 +1100
Subject: fix the eq settings in the manual

Change-Id: I4fa8537f31faef0d4f6f925476dcfb8b3336113b
---
 manual/appendix/config_file_options.tex | 25 ++++++++++---------------
 1 file changed, 10 insertions(+), 15 deletions(-)

(limited to 'manual/appendix/config_file_options.tex')

diff --git a/manual/appendix/config_file_options.tex b/manual/appendix/config_file_options.tex
index 44e8632ac2..8750147048 100644
--- a/manual/appendix/config_file_options.tex
+++ b/manual/appendix/config_file_options.tex
@@ -209,21 +209,16 @@
 %
       eq enabled    & on, off           & N/A\\
       eq precut     & 0 to 240          & 0.1~dB\\
-      eq band 0 cutoff & 0 to 32768     & Hz\\
-      eq band 1 cutoff & 0 to 32768     & Hz\\
-      eq band 2 cutoff & 0 to 32768     & Hz\\
-      eq band 3 cutoff & 0 to 32768     & Hz\\
-      eq band 4 cutoff & 0 to 32768     & Hz\\
-      eq band 0 q   & 0 to 64           & N/A\\
-      eq band 1 q   & 0 to 64           & N/A\\
-      eq band 2 q   & 0 to 64           & N/A\\
-      eq band 3 q   & 0 to 64           & N/A\\
-      eq band 4 q   & 0 to 64           & N/A\\
-      eq band 0 gain & -240 to 240      & 0.1~dB\\
-      eq band 1 gain & -240 to 240      & 0.1~dB\\
-      eq band 2 gain & -240 to 240      & 0.1~dB\\
-      eq band 3 gain & -240 to 240      & 0.1~dB\\
-      eq band 4 gain & -240 to 240      & 0.1~dB\\
+      eq low shelf filter & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 1 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 2 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 3 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 4 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 5 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 6 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 7 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq peak filter 8 & cutoff (in Hz), q (0 to 64), gain (-240 to 240)\\
+      eq high shelf filter & cutoff (in Hz), q (0 to 64), gain (-240 to 240 (0.1~dB))\\
 %
       dithering enabled & on, off       & N/A\\
 %
-- 
cgit v1.2.3

