From c81e1e1bf1addf05af62d14047fad3a3cfb4c76c Mon Sep 17 00:00:00 2001
From: Solomon Peachy <pizza@shaftnet.org>
Date: Sun, 26 Jul 2020 08:56:22 -0400
Subject: manual:  Strip out a few more archos-specific chunks

Change-Id: If875fc86888491d8b26d9090ae3ae778dc32aa31
---
 manual/appendix/config_file_options.tex | 24 +++---------------------
 1 file changed, 3 insertions(+), 21 deletions(-)

(limited to 'manual/appendix/config_file_options.tex')

diff --git a/manual/appendix/config_file_options.tex b/manual/appendix/config_file_options.tex
index e9604bdc33..74607b4507 100644
--- a/manual/appendix/config_file_options.tex
+++ b/manual/appendix/config_file_options.tex
@@ -11,9 +11,7 @@
     \toprule
     \rowcolor{tblhdrbgcolor}\tblhdrstrut\textbf{Setting} & \textbf{Allowed Values} & \textbf{Unit}\\
     \midrule\localendhead % endhead breaks with htlatex
-    volume      & \opt{masd}{$-78$ to +18}%
-                  \opt{masf}{$-100$ to +12}%
-                  \opt{iriverh100,iriverh300}{$-84$ to 0}%
+    volume      & \opt{iriverh100,iriverh300}{$-84$ to 0}%
                   \opt{ipodnano}{$-72$ to +6}%
                   \opt{ipodvideo,cowond2}{$-89$ to +6}%
                   \opt{iaudiom3,iaudiom5,iaudiox5}{$-73$ to +6}%
@@ -21,16 +19,12 @@
                   \opt{e200,e200v2,ipodcolor,mrobe100,vibe500,ipodnano2g}{$-74$ to +6}%
                   \opt{samsungyh}{$-128$ to 0}%
                                         & dB\\
-    bass        & \opt{masd}{$-15$ to +15}%
-                  \opt{masf}{$-12$ to +12}%
-                  \opt{iriverh100,iriverh300}{0 to +24}%
+    bass        & \opt{iriverh100,iriverh300}{0 to +24}%
                   \opt{ipod,mrobe100}{$-6$ to +9}%
                   \opt{iaudiom3,iaudiom5,iaudiox5,e200,e200v2,vibe500,fuzeplus,%
                        samsungyh}{$-24$ to +24}%
                                         & dB\\
-    treble      & \opt{masd}{$-15$ to +15}%
-                  \opt{masf}{$-12$ to +12}%
-                  \opt{iriverh100,iriverh300}{0 to +6}%
+    treble      & \opt{iriverh100,iriverh300}{0 to +6}%
                   \opt{ipod,mrobe100}{$-6$ to +9}%
                   \opt{iaudiom3,iaudiom5,iaudiox5,e200,e200v2,vibe500,fuzeplus,%
                        samsungyh}{$-24$ to +24}%
@@ -250,18 +244,6 @@
       }
     }%
 
-    \opt{masf}{
-      loudness      & 0 to 17           & N/A\\
-      superbass     & on, off           & N/A\\
-      auto volume   & off, 20ms, 2s, 4s, 8s
-                                        & N/A\\
-      mdb enable    & on,off            & N/A\\
-      mdb strength  & 0 to 127          & dB\\
-      mdb harmonics & 0 to 100          & \%\\
-      mdb center    & 20 to 300         & Hz\\
-      mdb shape     & 50 to 300         & Hz\\
-    }%
-
     \opt{lcd_bitmap}{
       peak meter release
                     & 1 to 126          & ?\\
-- 
cgit v1.2.3

