From 67a1db437f5dd5f095410a809e1d4122739b5bca Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Wed, 19 Oct 2011 06:02:35 +0000
Subject: Reviewed and updated recording samples rates in the manual. Fixes
 FS#12318.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@30802 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/recording_settings.tex | 15 ++++++++++-----
 1 file changed, 10 insertions(+), 5 deletions(-)

(limited to 'manual/configure_rockbox/recording_settings.tex')

diff --git a/manual/configure_rockbox/recording_settings.tex b/manual/configure_rockbox/recording_settings.tex
index 8fa152fde4..bddb4af0c8 100644
--- a/manual/configure_rockbox/recording_settings.tex
+++ b/manual/configure_rockbox/recording_settings.tex
@@ -41,25 +41,29 @@
 }
 
   \section{Frequency}
-   \nopt{sansa,ipodnano,ipodcolor,ipod4g}{
+   \nopt{ipodnano,ipodcolor,ipod4g}{
     Choose the recording frequency (sample rate).
+    \opt{c200,e200}
+        {24~kHz, 22.05~kHz and 16~kHz}
     \opt{iriverh100,iriverh300}
         {44.1~kHz, 22.05~kHz and 11.025~kHz}
     \opt{iaudiom3,iaudiom5,iaudiox5,vibe500}
         {88.2~kHz, 44.1~kHz, 22.05~kHz and 11.025~kHz}
     \opt{masf}
         {48~kHz, 44.1~kHz, 32~kHz, 24~kHz, 22.05~kHz and 16~kHz}
+    \opt{iriverh10}
+        {96~kHz, 88.2~kHz, 48~kHz, 44.1~kHz, 32~kHz and 8~kHz}
     \opt{gigabeats,ipodvideo}
         {48~kHz, 44.1~kHz, 32~kHz, 24~kHz, 22.05~kHz, 16~kHz, 12~kHz, %
         11.025~kHz and 8~kHz}
-    \opt{sansaAMS,ipodnano2g}
+    \opt{sansaAMS,ipodnano2g,c200v2,e200v2,fuze,fuzev2,fuzeplus,clipv1,clipv2,clipplus}
         {96~kHz, 88.2~kHz, 64~kHz, 48~kHz, 44.1~kHz, 32~kHz, 24~kHz, %
         22.05~kHz, 16~kHz, 12~kHz, 11.025~kHz and 8~kHz}
     are available. Higher sample rates use up more disk space, but give better
     sound quality.
     \opt{swcodec}{\note{The 11.025~kHz setting is not available when using %
       \setting{MPEG Layer~3} format.}
-    }%
+    }
     \opt{masf}{
       The frequency setting also determines which version of the MPEG standard
       the sound is recorded using:\\
@@ -69,11 +73,12 @@
     \opt{recording_digital}
       {\note{You cannot change the sample rate for digital recordings.}
     }
-   } % nopt sansa
+   } % nopt ipodnano,ipodcolor,ipod4g
    \opt{sansa}{
+     \nopt{c200,e200,c200v2,e200v2,fuze,fuzev2,fuzeplus,clipv1,clipv2,clipplus}
       Recordings can only be made at a 22.05~kHz frequency (sample rate)
       on this \dap. 
-   } % opt sansa
+   } % prepared for all sansas not handled above, e.g. sansaview
    \opt{ipodnano,ipodcolor,ipod4g}{
       Recordings can only be made at a 44.1~kHz frequency (sample rate)
       on this \dap. 
-- 
cgit v1.2.3

