From a09152b1284d81f5454d6ae0b25081ef59aa5072 Mon Sep 17 00:00:00 2001
From: Szymon Dziok <b0hoon@o2.pl>
Date: Thu, 15 Apr 2010 18:35:41 +0000
Subject: Packard Bell Vibe 500: Add a part of the manual (no plugin keymaps
 yet).

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25652 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/recording_settings.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'manual/configure_rockbox/recording_settings.tex')

diff --git a/manual/configure_rockbox/recording_settings.tex b/manual/configure_rockbox/recording_settings.tex
index aa469aca03..14a53e9b4a 100644
--- a/manual/configure_rockbox/recording_settings.tex
+++ b/manual/configure_rockbox/recording_settings.tex
@@ -46,7 +46,7 @@
     Choose the recording frequency (sample rate).
     \opt{masf}{48~kHz, 44.1~kHz, 32~kHz, 24~kHz, 22.05~kHz, 16~kHz}
     \opt{h100,h300}{44.1~kHz, 22.05~kHz and 11.025~kHz}
-    \opt{x5}{88.2~kHz, 44.1~kHz, 22.05~kHz and 11.025~kHz}
+    \opt{x5,vibe500}{88.2~kHz, 44.1~kHz, 22.05~kHz and 11.025~kHz}
     \opt{sansaAMS}{96~kHz, 88.2~kHz, 64~kHz, 48~kHz, 44.1~kHz, 32~kHz, 24~kHz, %
         22.05~kHz, 16~kHz, 12~kHz, 11.025~kHz and 8~kHz}
     \opt{gigabeats}{48~kHz, 44.1~kHz, 32~kHz, 24~kHz, 22.05~kHz, 16~kHz, 12~kHz, %
@@ -75,8 +75,8 @@
   Choose the source of the recording. The options are: 
   \opt{recorder,recorderv2fm,h100}{\setting{SPDIF (digital)}, }%
   \nopt{ipodnano,ipodvideo}{\setting{Mic}\nopt{radio}
-    {\nopt{recorder,m5,ipod4g,ipodcolor}{,} and }}%
-  \nopt{sansa,sansaAMS}{\nopt{ipodnano,ipodvideo,recorder,m5,ipod4g,ipodcolor}%
+    {\nopt{recorder,m5,ipod4g,ipodcolor,vibe500}{,} and }}%
+  \nopt{sansa,sansaAMS}{\nopt{ipodnano,ipodvideo,recorder,m5,ipod4g,ipodcolor,vibe500}%
     {, }\setting{Line In}}%
   \nopt{radio}{.}
   \opt{radio}{and {\setting{FM Radio}}. For more information on recording from the radio
-- 
cgit v1.2.3

