From 9ca8bd64cd8b9734a82116e0037f4555c6ec3582 Mon Sep 17 00:00:00 2001
From: Amaury Pouly <amaury.pouly@gmail.com>
Date: Sat, 20 Aug 2016 21:31:12 +0100
Subject: manual: document 3D enhancement

3D "enhancement" is available on all imx233 platform, and also on platforms
with the WM8978 codec (gigabeats) and WM8750 codec (MPIO HD 200/300). I used
different texts for different codecs because (in theory) they do different
"things".

Change-Id: I62ecb075f7594427491b6be83cfa80f763566aba
---
 manual/configure_rockbox/sound_settings.tex | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

(limited to 'manual/configure_rockbox/sound_settings.tex')

diff --git a/manual/configure_rockbox/sound_settings.tex b/manual/configure_rockbox/sound_settings.tex
index caebd3c37c..f9f0a747dd 100644
--- a/manual/configure_rockbox/sound_settings.tex
+++ b/manual/configure_rockbox/sound_settings.tex
@@ -189,6 +189,20 @@ change to customise your listening experience.
   the effect of widening the stereo field. A value of 100\% will leave the
   stereo field unaltered.
 
+\opt{depth_3d}{
+  \section{3D Enhancement}
+  3D Enhancement increases the perceived separation between the left and right
+  channels.
+  \opt{IMX233}{%
+    It works by subtracting a portion of the opposite channel's content for each
+    channel. This setting controls the amount of opposite channel content that
+    is subtracted. A value of 0dB leaves the audio signal unmodified.}%
+  \opt{HAVE_WM8750,HAVE_WM8978}{%
+    This settings controls the degree of stereo expansion. A value of 0\%
+    leaves the audio signal unmodified.
+  }%
+}
+
 \opt{masf}{
   \section{Loudness}
   When listening at low volumes, the ear will tend to make bass and treble
-- 
cgit v1.2.3

