From f498d53d72007124049cf72ccccf3435abb097fe Mon Sep 17 00:00:00 2001
From: Dominik Riebeling <Dominik.Riebeling@gmail.com>
Date: Sun, 7 Dec 2008 23:00:15 +0000
Subject: Rename h100 manual name "h1xx" to "h100" to be in line with other
 players.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@19361 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/sound_settings.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'manual/configure_rockbox/sound_settings.tex')

diff --git a/manual/configure_rockbox/sound_settings.tex b/manual/configure_rockbox/sound_settings.tex
index c0116e40d7..60fc127e99 100644
--- a/manual/configure_rockbox/sound_settings.tex
+++ b/manual/configure_rockbox/sound_settings.tex
@@ -19,7 +19,7 @@ change to customise your listening experience.
   The volume can be adjusted from a
   \opt{player}{minimum of -78 dB to a maximum of +18 dB.}%
   \opt{recorder,recorderv2fm,ondio}{minimum of -100 dB to a maximum of +12 dB.}%
-  \opt{h1xx,h300}{minimum of -84 dB to a maximum of 0 dB.}%
+  \opt{h100,h300}{minimum of -84 dB to a maximum of 0 dB.}%
   \opt{x5,m5,ipod3g,ipod4g,gigabeatf,mrobe100}{minimum of -73 dB to a maximum of +6 dB.}%
   \opt{ipodnano}{minimum of -72 dB to a maximum of +6 dB.}%
   \opt{ipodvideo}{minimum of -57 dB to a maximum of +6 dB.}%
@@ -28,12 +28,12 @@ change to customise your listening experience.
 
 \section{Bass}
   This setting emphasises
-  \nopt{h1xx,h300}{or suppresses}
+  \nopt{h100,h300}{or suppresses}
   the lower (bass) frequencies in the sound. A value of 0 dB means that bass
   sounds are unaltered (flat response).
   \opt{masd}{The minimum setting is -15 dB and the maximum is 15 dB.}%
   \opt{masf}{The minimum setting is -12 dB and the maximum is 12 dB.}%
-  \opt{h1xx,h300}{The minimum setting is 0 dB and the maximum is 24 dB.}%
+  \opt{h100,h300}{The minimum setting is 0 dB and the maximum is 24 dB.}%
   \opt{ipodnano,ipodcolor}{The minimum setting is -6 dB and the maximum is 9 dB.}%
   \opt{ipodvideo}{The minimum setting is -12 dB and the maximum is 12 dB.}%
   \opt{x5,sansa,h10,h10_5gb}{The minimum setting is -24 dB and the maximum is 24 dB.}
@@ -48,12 +48,12 @@ change to customise your listening experience.
 
 \section{Treble}
   This setting emphasises
-  \nopt{h1xx,h300}{or suppresses}
+  \nopt{h100,h300}{or suppresses}
   the higher (treble) frequencies in the sound. A value of 0 dB means that
   treble sounds are unaltered (flat response).
   \opt{masd}{The minimum setting is -15 dB and the maximum is 15 dB.}%
   \opt{masf}{The minimum setting is -12 dB and the maximum is 12 dB.}%
-  \opt{h1xx,h300}{The minimum setting is 0 dB and the maximum is 6 dB.}%
+  \opt{h100,h300}{The minimum setting is 0 dB and the maximum is 6 dB.}%
   \opt{ipodnano,ipodcolor}{The minimum setting is -6 dB and the maximum is 9 dB.}%
   \opt{ipodvideo}{The minimum setting is -12 dB and the maximum is 12 dB.}%
   \opt{x5,sansa,h10,h10_5gb}{The minimum setting is -24 dB and the maximum is 24 dB.}
-- 
cgit v1.2.3

