From 10023adf727391cd165be7b5290e83a4710d0129 Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Mon, 29 Mar 2010 17:58:17 +0000
Subject: Add new section 'Optimising battery runtime' to the manual
 (FS#11148).

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25382 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index d2eb992b89..af7695ed48 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -152,7 +152,7 @@ This sub menu relates to limits in the Rockbox operating system.
 }
 
 \opt{accessory_supply}{
-\subsection{Accessory Power Supply}
+\subsection{\label{ref:AccessoryPowerSupply}Accessory Power Supply}
 This option turns the accessory power supply \setting{On} and \setting{Off}.
 The Apple accessory protocol has been partially implemented in Rockbox, and
 thus there is a reasonable chance that your favourite accessory will work.
@@ -162,7 +162,7 @@ this option \setting{On}. If it is not required, then turning this setting
 }
 
 \opt{lineout_poweroff}{
-\subsection{Line Out}
+\subsection{\label{ref:LineoutOnOff}Line Out}
 This option turns the \dap{}'s line-out \setting{On} and \setting{Off}. On some 
 devices an enabled line-out will consume some power even if not used. If it is 
 not required, then turning this setting \setting{Off} will save battery and 
-- 
cgit v1.2.3

