From 569933f6465e369c2bc69a46cf704fcfa6e80765 Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Tue, 23 Jan 2007 21:19:11 +0000
Subject: Remove the disk poweroff setting from the manual and make some minor
 tweaks

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@12096 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 52 ++++++++++++-----------------
 1 file changed, 22 insertions(+), 30 deletions(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index 1d8bfdc304..984c5ee202 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -2,7 +2,8 @@
 \section{\label{ref:SystemOptions}System Options}
 
 \subsection{Battery}
-    Options relating to the batteries in the \dap.
+    Options relating to the \opt{archos}{batteries}\nopt{archos}{battery}%
+    in the \dap.
   \begin{description}
     \item [Battery Capacity: ]This setting can be used to tell Rockbox what
       capacity (in mAh) of battery is being used inside it. The default is
@@ -40,27 +41,21 @@
       hard disk after it is idle for a certain amount of time. This setting
       controls the amount of time between the last user activity and the time
       that the disk spins down. This idle time is only affected by user
-      activity, like navigating through file browser. When the hard disk spins
-      up to fill the audio buffer, it automatically spins down afterwards.
-      
-    \opt{recorder,h1xx,h300,x5}{
-      \item [Disk Poweroff: ]This setting controls whether the disk is powered
-      off or only set to ``sleep'' when spun down. If this setting is set to
-      \setting{Yes}, the disk will power off. If set to \setting{No}, the disk
-      will enter ``sleep'' mode. Power off uses less power but takes slightly
-      longer to spin-up.
-    }
+      activity, like navigating through the \setting{File Browser}. When the
+      hard disk spins up to fill the audio buffer, it automatically spins down
+      afterwards.
+
     \opt{SWCODEC}{
-    \item [Directory Cache: ]Rockbox has the ability to scan the contents of
-      your drive in the background and save those contents to a cache in RAM.
-      The \setting{Directory Cache} takes a small amount of memory away from 
-      Rockbox that would otherwise be used to buffer music, but it speeds up 
-      navigation by eliminating the slight pause between the time a navigation 
-      button is pressed and the time Rockbox responds. Turning this setting 
-      \setting{On} activates the directory cache, and turning it \setting{Off} 
-      deactivates the directory cache.
+    \item [Directory Cache: ]Rockbox has the ability to cache the contents of
+      your drive in RAM. The \setting{Directory Cache} takes a small amount of
+      memory away from Rockbox that would otherwise be used to buffer music,
+      but it speeds up navigation in the \setting{File Browser} by eliminating
+      the slight pause between the time a navigation button is pressed and the
+      time Rockbox responds. Turning this setting \setting{On} activates the
+      directory cache, and turning it \setting{Off} deactivates the directory
+      cache.
       \note{The first time you set the directory cache to \setting{On},
-      Rockbox will request a reboot of the \dap\ and upon restarting take a few
+      Rockbox will request a reboot of the \dap{} and upon restarting take a few
       minutes to scan the drive. Thereafter, the directory cache will work in the
       background.}
     }
@@ -77,9 +72,9 @@
 }
 
 \subsection{Idle Poweroff}
-Rockbox can be configured to turn off power after the unit has been idle for a 
-defined number of minutes. The \dap{} is idle when playback is stopped or 
-paused. It is not idle while the USB or charger is connected, or while 
+Rockbox can be configured to turn off power after the unit has been idle for a
+defined number of minutes. The \dap{} is idle when playback is stopped or
+paused. It is not idle while the USB or charger is connected, or while
 recording. Settings are either \setting{Off} or \setting{1} to \setting{10}
 minutes in 1 minute steps. Then \setting{15,30,45} and \setting{60} minutes are
 available.
@@ -87,8 +82,7 @@ available.
 This option lets you power off your \dap{} after playing for a given time. Can
 be set from \setting{Off} to 5 hours in 5 minute steps.
 \opt{recorderv2fm}{This setting is reset on boot. Using this option
-  disables the \setting{Wake up alarm} (see below).}
-\opt{recorderv2fm}{
+  disables the \setting{Wake up alarm} (see below).
   \subsection{Wake Up alarm}
     This option turns the \dap{} off and then starts it up again at the 
     specified time. This is most useful when combined with the \setting{Resume}
@@ -107,9 +101,9 @@ This sub menu relates to limits in the Rockbox operating system.
   \begin{description}
     \item [Max files in dir browser: ]This setting controls the limit on
     the number of files that you can put in any particular directory in the
-    file browser. You can configure the size to be between 50 and 10,000 files
-    in steps of 50 files. The default is 400. Higher values will shorten the
-    music buffer, so you should increase this setting \emph{only} if you have
+    \setting{File Browser}. You can configure the size to be between 50 and
+    10,000 files in steps of 50. The default is 400. Higher values will shorten
+    the music buffer, so you should increase this setting \emph{only} if you have
     directories with a large number of files.
 
     \item [Max playlist size: ]This setting controls the maximum size of 
@@ -151,5 +145,3 @@ This sub menu relates to limits in the Rockbox operating system.
     \item LAN party computer $\rightarrow$ \dap $\rightarrow$ human
     \end{itemize}
 }
-
-
-- 
cgit v1.2.3

