From 6a96037d09c99041bae87ae7c7a5189adafd7408 Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Sun, 9 May 2010 21:03:30 +0000
Subject: Add non-breaking spaces to mA, mAh, MB and GB. Add playertype for
 iPod Video when describing the different variants.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25921 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 34 ++++++++++++++---------------
 1 file changed, 17 insertions(+), 17 deletions(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index 025496efd1..e8dc2310f9 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -15,21 +15,21 @@
   \begin{description}
     \item [Battery Capacity.] This setting can be used to tell Rockbox what
       capacity (in mAh) the battery being used has. The default is
-      \opt{player,recorder}{1500mAh}%
-      \opt{recorderv2fm}{2200mAh}%
-      \opt{ondiosp,ondiofm,vibe500}{1000mAh}%
-      \opt{h100,h300}{1300mAh}%
-      \opt{ipodmini}{400mAh (1G) or 630mAh (2G)}%
-      \opt{ipodcolor}{700mAh}%
-      \opt{ipodnano}{300mAh}%
-      \opt{ipodvideo}{400mAh (30GB) or 600mAh (60/80GB)}%
-      \opt{ipod4g}{630mAh}%
-      \opt{ipod3g}{630mAh}%
-      \opt{ipod1g2g}{1200mAh}%
-      \opt{m5,x5}{950mAh}%
-      \opt{gigabeatf}{2000mAh}%
-      \opt{gigabeats}{700mAh}%
-      \opt{cowond2}{1600mAh}%
+      \opt{player,recorder}{1500~mAh}%
+      \opt{recorderv2fm}{2200~mAh}%
+      \opt{ondiosp,ondiofm,vibe500}{1000~mAh}%
+      \opt{h100,h300}{1300~mAh}%
+      \opt{ipodmini}{400~mAh (1G) or 630~mAh (2G)}%
+      \opt{ipodcolor}{700~mAh}%
+      \opt{ipodnano}{300~mAh}%
+      \opt{ipodvideo}{400~mAh (30~GB) or 600~mAh (60/80~GB)}%
+      \opt{ipod4g}{630~mAh}%
+      \opt{ipod3g}{630~mAh}%
+      \opt{ipod1g2g}{1200~mAh}%
+      \opt{m5,x5}{950~mAh}%
+      \opt{gigabeatf}{2000~mAh}%
+      \opt{gigabeats}{700~mAh}%
+      \opt{cowond2}{1600~mAh}%
       , which is the capacity value for the standard
       \opt{archos}{batteries}\nopt{archos}{battery} shipped with the \dap.
         Rockbox uses this value for runtime estimation, not battery percentage
@@ -39,7 +39,7 @@
       \opt{iaudio}{Rockbox does not automatically distinguish between the
         ``L'' models and the ``simple'' models which determine the default
         value. If your dap{} is an \opt{m5}{M5L}\opt{x5}{X5L} set the value
-        to 2250mAh for more accuracy in the runtime estimation.}
+        to 2250~mAh for more accuracy in the runtime estimation.}
       \opt{ipod,sansa}{This value is fairly meaningless in the \playerman{}
         family at present, and work is on-going into finding a better way to
         determine battery life.}
@@ -52,7 +52,7 @@
       \opt{h300,ipodnano2g}{
       \item [Charge During USB Connection.] This option lets you control whether
         the \dap{} should charge during the USB connection and hence draw the
-        full 500mA. Turning it \setting{Off} is recommended if the dap{} is
+        full 500~mA. Turning it \setting{Off} is recommended if the dap{} is
         connected through an unpowered USB hub or a laptop port.
       }
 
-- 
cgit v1.2.3

