From 98755fd49362a0f9ae0f732b1575b484f75cf8d8 Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Sun, 22 Nov 2009 11:41:14 +0000
Subject: Only the H300 and Nano 2G have the charge from USB option at present.
 Thanks to jmdennis on the forums for pointing out, and Torne Wuff for the
 info on which players it is present for.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@23695 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index 0651d61f7d..07fb05bb37 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -48,7 +48,7 @@
         is currently used in the \dap{}. The two supported battery types are
         ``Alkaline'' or ``NiMH''.}
 
-      \opt{usb_charging}{
+      \opt{h300,ipodnano2g}{
       \item [Charge During USB Connection.] This option lets you control whether
         the \dap{} should charge during the USB connection and hence draw the
         full 500mA. Turning it \setting{Off} is recommended if the dap{} is
-- 
cgit v1.2.3

