From 09b2e589989a356cefd0437bd391e0032d34a664 Mon Sep 17 00:00:00 2001
From: Dominik Riebeling <Dominik.Riebeling@gmail.com>
Date: Mon, 30 Jul 2007 18:32:48 +0000
Subject: Gigabeat needs to be power-cycled after bootloader installation.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@14078 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/gigabeat_install.tex | 10 ++++++++++
 1 file changed, 10 insertions(+)

(limited to 'manual/getting_started/gigabeat_install.tex')

diff --git a/manual/getting_started/gigabeat_install.tex b/manual/getting_started/gigabeat_install.tex
index 0497d7f347..5d225c7f76 100644
--- a/manual/getting_started/gigabeat_install.tex
+++ b/manual/getting_started/gigabeat_install.tex
@@ -20,3 +20,13 @@ of the original file.
   Make sure the spelling is correct.
 \end{itemize}
 
+\warn{After installing the bootloader you \emph{need} to power-cycle the 
+\dap{} by doing the following steps. Failure to do so may result in problems.}
+\begin{itemize}
+\item Eject / unmount USB drive and unplug the USB cable.
+\item Unplug any power adapter.
+\item Hold the \ButtonPower{} button to turn off the \dap{}.
+\item Slide the battery switch located on the bottom of the \dap{} from 
+    `on' to `off'
+\item Slide the battery switch back from `off' to `on'
+\end{itemize}
-- 
cgit v1.2.3

