From 42ef5b0c88f92418c79e7414063c808b7c36a9be Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Tue, 17 Feb 2009 23:19:01 +0000
Subject: Reorganise/partially rewrite the installation chapter to present
 Rockbox Utility as the preferred installation method, and don't have
 important information only under manual install.  For now retain manual
 install as a subsection.  Patch originally in FS#9895

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@20034 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/h10_install.tex | 19 -------------------
 1 file changed, 19 deletions(-)

(limited to 'manual/getting_started/h10_install.tex')

diff --git a/manual/getting_started/h10_install.tex b/manual/getting_started/h10_install.tex
index bb212a6504..ff72f6661e 100644
--- a/manual/getting_started/h10_install.tex
+++ b/manual/getting_started/h10_install.tex
@@ -1,22 +1,3 @@
-\subsubsection{UMS and MTP}
-The \playertype{} can be connected to a computer in two different modes:
-\begin{itemize}
-  \item Universal Mass Storage (UMS): In this mode, it will appear on your computer as a regular disk. This mode works with all major operating systems, including Windows, Linux and Mac OS X.
-  \item Media Transfer Protocol (MTP): In this mode, it will appear on your computer as a Media Device. MTP was created by Microsoft for use with DAPs and only works with Windows XP and Media Player 10.
-\end{itemize}
-The \playerlongtype{} is \opt{h10}{only available as a MTP device, but}\opt{h10_5gb}{available as both a MTP and as a UMS device, depending on where and when you bought it. You can tell which you have by how it appears when you connect it to a computer. If it appears as a regular disk then it is UMS. If it appears as a Media Device on Windows XP, or if it does not appear at all on other operating systems, then it is MTP. Even if you have a MTP \dap{}, it} can be forced into UMS mode using the UMS trick.
-
-\subsubsection{UMS mode and the UMS trick}
-It is possible to force a MTP \playertype{} to start up in UMS mode using the following procedure:
-\begin{enumerate}
-  \item Ensure the \dap{} is fully powered off by \opt{h10}{using a pin to push the small reset button inside the hole between the Hold switch and remote control connector.}\opt{h10_5gb}{removing the battery and putting it back in again.}
-  \item Connect your \playertype{} to the computer using the data cable.
-  \item Hold \ButtonRight{} and push \ButtonPower{} to turn the \dap{} on.
-  \item Continue holding \ButtonRight{} until the USB Connected screen appears.
-  \item The \dap{} will now appear as a regular disk on your computer.
-\end{enumerate}
-\note{Once Rockbox has been installed, when you shut down your \dap{} from Rockbox it will totally power the player off so step 1 is no longer necessary.}
-
 \subsubsection{Installation}
 \begin{enumerate}
   \item Download 
-- 
cgit v1.2.3

