From 4c6b94551e5e8eef36f6919d3992dc9f331562c1 Mon Sep 17 00:00:00 2001
From: Rafaël Carré <rafael.carre@gmail.com>
Date: Thu, 20 May 2010 18:34:05 +0000
Subject: fuzev2: make manual build

Use the same info than Clipv1/v2 to warn about the version
(the path in OF menu to check the version has just one more component on Fuze)

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@26205 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 20 +++++++-------------
 1 file changed, 7 insertions(+), 13 deletions(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 9e6b6feaa7..2717b5cfe5 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -11,7 +11,7 @@ before beginning there are a few things it is important to know.
 follow the instructions at 
 \url{http://www.rockbox.org/twiki/bin/view/Main/SansaE200RInstallation}.}}
 
-\opt{ipodnano,ipodnano2g,ipodvideo,e200,c200,e200v2,clipv1,clipv2,cowond2,fuze}{
+\opt{ipodnano,ipodnano2g,ipodvideo,e200,c200,e200v2,clipv1,clipv2,cowond2,fuze,fuzev2}{
 \begin{description}  
 \item[Supported hardware versions.] 
     \opt{ipodnano,ipodnano2g}{
@@ -43,19 +43,13 @@ follow the instructions at
     v2 firmware begins with 03. Make sure that you are following the
     instructions from the correct manual.
 }
-  \opt{clipv1,clipv2}{
+  \opt{clipv1,clipv2,fuze,fuzev2}{
     The \playertype{} is available in multiple versions, and you need to make
-    sure which you have by checking the Sandisk firmware version number under 
-    Settings $\rightarrow$ Info. The v1 firmware is named 01.xx.xx, while the
-    v2 firmware begins with 02. Make sure that you are following the
-    instructions from the correct manual.
-}
-  \opt{fuze}{
-    The \playertype{} is available in multiple versions, not all of which
-    run Rockbox.  Rockbox doesn't run on the newer v2 models. They can be
-    identified by checking the Sandisk firmware version number under 
-    System Settings $\rightarrow$ System Info. The v1 firmware is named
-    01.xx.xx, while the v2 firmware begins with 02.
+    sure which you have by checking the Sandisk firmware version number under
+    Settings $\rightarrow$ \opt{fuze,fuzev2}{System Settings $\rightarrow$}
+    Info. The v1 firmware is named 01.xx.xx, while the v2 firmware begins with
+    02. Make sure that you are following the instructions from the correct
+    manual.
 }
   \opt{cowond2}{
     Rockbox runs on all \playerman{} \playertype{} and \playertype{}+ variants
-- 
cgit v1.2.3

