From a8b5589523a0be2f26a22607e5c0e12382a64f4e Mon Sep 17 00:00:00 2001
From: Szymon Dziok <b0hoon@o2.pl>
Date: Wed, 15 Oct 2014 16:23:34 +0200
Subject: Manual for the Samsung YH920/YH925.

Change-Id: I2db0023cae585e9c9517da9ed2e9de6195081ce2
---
 manual/getting_started/samsungyh_install.tex | 12 ++++++++++++
 1 file changed, 12 insertions(+)
 create mode 100644 manual/getting_started/samsungyh_install.tex

(limited to 'manual/getting_started/samsungyh_install.tex')

diff --git a/manual/getting_started/samsungyh_install.tex b/manual/getting_started/samsungyh_install.tex
new file mode 100644
index 0000000000..1c7a65bc87
--- /dev/null
+++ b/manual/getting_started/samsungyh_install.tex
@@ -0,0 +1,12 @@
+% $Id: %
+\subsubsection{Installation}
+\begin{enumerate}
+  \item Download 
+  \opt{samsungyh920}{\url{http://download.rockbox.org/bootloader/samsung/yh920/PP5020.mi4}}
+  \opt{samsungyh925}{\url{http://download.rockbox.org/bootloader/samsung/yh925/FW_YH925.mi4}}
+  \item Connect your \playertype{} to the computer using UMS mode.
+  \item Rename the \originalfirmwarefilename{} file to \fname{OF.mi4} in the \fname{System} directory on your \playertype{}.
+    \note{You should keep a safe backup of this file for use if you ever wish to switch back to the \playerman{} firmware.}
+    \note{If you cannot see the \fname{System} directory, you will need to make sure your operating system is configured to show hidden files and directories.}
+  \item Copy the \originalfirmwarefilename{} file you downloaded to the \fname{System} directory on your \dap{}.
+\end{enumerate}
-- 
cgit v1.2.3

