From 792f64e64eaddb55d94c43aa5f44e738b6c7614b Mon Sep 17 00:00:00 2001
From: Nils Wallménius <nils@rockbox.org>
Date: Sat, 22 Jul 2006 09:46:31 +0000
Subject: Main menu chapter: broke out recording and fmradio sections to their
 own files. Recording: added ondio and x5 keys corrected errors in keymaps and
 opted out settings that are unavailable on some targets. FMradio: added x5
 and ondio keys.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@10281 a1c6a512-1295-4272-9138-f99709370657
---
 manual/main_menu/main.tex | 284 +---------------------------------------------
 1 file changed, 3 insertions(+), 281 deletions(-)

(limited to 'manual/main_menu/main.tex')

diff --git a/manual/main_menu/main.tex b/manual/main_menu/main.tex
index 7447a63438..bc486c5c2d 100644
--- a/manual/main_menu/main.tex
+++ b/manual/main_menu/main.tex
@@ -118,287 +118,10 @@ headphones and when connected to an external amplifier.  See the section on
 for more details. 
 }
 
-      
-\opt{CONFIG_TUNER}{
-  \section{\label{ref:FMradio}FM Radio}  
-  \opt{x5}{\note{Not currently Implemented on X5}}
+\opt{CONFIG_TUNER}{\input{main_menu/fmradio.tex}}
 
-  \screenshot{main_menu/images/ss-fm-radio-screen}{The FM radio screen}{}
-  
-  This menu option switches to the radio screen.
-  
-  The FM radio has the ability \opt{HAVE_RECORDING}{to record and } to
-  remember station frequency settings (presets).
+\opt{HAVE_RECORDING}{\input{main_menu/recording.tex}}
 
-  \opt{recorderv2fm,ondio}{   
-    \begin{table}
-      \begin{btnmap}{}{}
-          \ButtonLeft, \ButtonRight 
-          & Change frequency in 0.1 MHz steps.\\
-          & For automatic station seek, hold \ButtonLeft/\ButtonRight\ %
-            for a little longer. \\
-          %
-          \ButtonUp, \ButtonDown    
-          & Change volume \\
-          %
-          \opt{RECORDER_PAD}{
-            \ButtonPlay      & \emph{(EXPERIMENTAL)}\\
-            & freezes all screen updates.May enhance radio reception
-              in some cases.\\
-          }
-          \opt{RECORDER_PAD}{\ButtonOn}\opt{ONDIO_PAD}{\ButtonOff}
-          & Leave the radio screen with the radio playing \\
-          %
-	   \opt{RECORDER_PAD}{\ButtonOff}\opt{ONDIO_PAD}{hold \ButtonOff}
-          & Back to Main Menu.\\
-       \end{btnmap}
-    \end{table}
-  }
-  \fixme{Add Radio recording and Preset keys to FM Recorder and Ondio FM}
-  
-  \opt{h1xx,h300,x5}{
-    \begin{table}
-      \begin{btnmap}{}{}
-          \ButtonLeft, \ButtonRight & Change frequency in 0.1 MHz steps. \\
-          Hold \ButtonLeft, \ButtonRight 
-                             & Seeks to next station or preset\\
-          %
-          \ButtonUp, \ButtonDown 
-                             & Change volume \\
-          %
-          \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOn}
-          \opt{IAUDIO_X5_PAD}{\fixme{TBD}}
-                             & Mutes radio playback \\
-          %
-          \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{Hold \ButtonOn}
-          \opt{IAUDIO_X5_PAD}{\fixme{TBD}}
-          & Switches between SCAN and PRESET mode.\\
-          %
-          \ButtonSelect      & Opens a list of radio presets. You can view 
-                               all the presets that you have, and switch to 
-                               the station.\\
-          Hold \ButtonSelect & Displays the FM radio settings menu.\\
-          %
-          \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonMode}
-          \opt{IAUDIO_X5_PAD}{\fixme{TBD}}
-          %
-                             & Keeps radio playing and returns to the main
-                               menu. You can then press OFF/STOP to browse 
-                               the file tree while listening to the radio\\
-          %
-          \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOff}
-          \opt{IAUDIO_X5_PAD}{\fixme{TBD}}
-                             & Stops the radio and returns to Main Menu.\\
-       \end{btnmap}
-    \end{table}
-  }
-  
-  \begin{description}
-    
-  \item[Saving a preset:]
-    Up to 32 of your favourite stations can be saved as presets. 
-    Press
-    \opt{RECORDER_PAD}{\ButtonFOne}
-    \opt{ONDIO_PAD}{\ButtonMenu}
-    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_X5_PAD}{\ButtonSelect}
-    to go to the menu, then select 
-    \opt{recorderv2fm,ondio}{``Save preset''.}
-    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_X5_PAD}{``Add preset''}
-    Enter the name (maximum number of characters is 32). 
-    \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{Press \ButtonOn\ to save.}
-    \opt{IAUDIO_X5_PAD}{Press \fixme{TBD} to save.}
-    
-  \item[Selecting a preset:]
-    \opt{ONDIO_PAD,RECORDER_PAD}
-       {         
-         Press \opt{RECORDER_PAD}{\ButtonFTwo}\opt{ONDIO_PAD}{\fixme{FixMe}}
-         to go to the preset list. Use \ButtonUp\ and \ButtonDown\ to 
-         move the cursor and then press 
-         \opt{RECORDER_PAD}{\ButtonPlay}\opt{ONDIO_PAD}{\fixme{FixMe}}
-         to select. Use \ButtonLeft\ to leave the preset without selecting
-         anything.
-       }
-     \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_X5_PAD}
-        {
-          Press \ButtonSelect\ to go to the preset list. 
-          Use \ButtonUp\ and \ButtonDown\ to move the cursor and then 
-          press \ButtonSelect\ to select. Use \ButtonLeft\ to leave the
-          preset without selecting anything.
-        }
-            
-  \item[Removing a preset:]
-     \opt{ONDIO_PAD,RECORDER_PAD}{
-        Press \opt{RECORDER_PAD}{\ButtonFOne}\opt{ONDIO_PAD}{\fixme{FixMe}}
-        to go to the menu, then select ``Remove preset''.
-      }
-      \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IAUDIO_X5_PAD}{
-        Press \ButtonSelect\ to go to the preset list. Use \ButtonUp\ 
-        and \ButtonDown\ to move the cursor and then Hold \ButtonSelect\ 
-        on the preset to that you wish to remove, then select ``Remove preset.''
-      }
-     
-      \opt{RECORDER_PAD}{
-          \item[Recording:]
-            Press \ButtonFThree\ to start recording the currently playing 
-            station. Press \ButtonOff\ to stop recording. Press \ButtonPlay\ 
-            again to seamlessly start recording to a new file. The settings
-            for the recording can be changed in the \ButtonFOne\ menu before
-            starting the recording. See page \pageref{ref:Recordingsettings} 
-            for details of recording settings.
-          }
-  \end{description}
-  \note{The radio will turn off when starting playback of an audio file.}
-}
-
-\opt{HAVE_RECORDING}{
-  \section{\label{ref:Recording}Recording} 
-  \opt{x5}{\note{Not Implemented on X5 yet}}
-  \subsection{\label{ref:Whilerecordingscreen}While Recording Screen}
-  \screenshot{main_menu/images/ss-while-recording-screen}{The while recording screen}{}
-  Entering the ``Recording'' option in the Main menu launches the recording 
-    application. The screen shows the time elapsed and the size of the file being 
-    recorded. A peak meter is present to allow you set Gain correctly.
-  \opt{MASCODEC}{The frequency, channels and quality}
-  \opt{SWCODEC}{The frequency and channels} settings are shown on the last line.
-  
-  The controls for this screen are:
-  
-    \begin{table}
-      \begin{btnmap}{}{}
-        \ButtonLeft & Decreases Gain \\
-        %
-        \ButtonRight & Increases Gain \\
-        %
-        \opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOn}
-        \opt{ONDIO_PAD,IAUDIO_X5_PAD,IPOD_4G_PAD}{\fixme{FixMe}} & Starts recording.  \\
-        & While recording: button closes the current file and opens a new one.\\
-        %
-        \opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonOff} 
-        \opt{ONDIO_PAD,IAUDIO_X5_PAD,IPOD_4G_PAD}{\fixme{FixMe}} & Exits Recording Screen.\\
-        & While recording: Stop recording \\
-        %
-        \opt{RECORDER_PAD}{\ButtonFOne}
-        \opt{ONDIO_PAD}{\ButtonMenu}
-        \opt{IPOD_4G_PAD,IAUDIO_X5_PAD}{Hold \ButtonSelect} 
-        \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonMode}
-        & Opens Recording Settings screen (see below) \\
-        %
-        \opt{RECORDER_PAD}{
-          \ButtonFTwo & Quick menu for recording settings. A quick press will 
-          leave the screen up (press {\ButtonFTwo} again to exit),while holding 
-          it will close the screen when you release it. \\
-        }
-        %
-        \opt{IRIVER_H100_PAD,IRIVER_H300_PAD,IPOD_4G_PAD,IAUDIO_X5_PAD}{
-          \ButtonSelect & Quick menu for recording settings. \\
-        }
-        %
-        \opt{RECORDER_PAD}{
-          \ButtonFThree & Quick menu for source setting. \\
-          & Quick/hold works as for {\ButtonFTwo}. \\
-          & While recording: Start a new recording file \\
-        }
-      \end{btnmap}
-  \end{table}
-  
-  \subsection{\label{ref:Recordingsettings}Recording Settings}
-  \screenshot{main_menu/images/ss-recording-settings}{The recording settings screen}{}
-  
-  \opt{MASCODEC}{
-    \begin{description}
-    \item[Quality:]
-      Choose the quality here (0 to 7). Default is 5, best quality is 7, 
-      smallest file size is 0. This setting effects how much your sound 
-      sample will be compressed. Higher quality settings result in larger 
-      MP3 files.
-      
-      The quality setting is just a way of selecting an average bit rate, 
-      or number of  bits per second, for a recording.  When  this setting 
-      is lowered, recordings are compressed more (meaning worse sound quality), 
-      and the average bitrate changes as follows.
-    \end{description}
-    
-    \begin{table}[h!]
-      \begin{center}
-        \begin{tabularx}{0.75\textwidth}{lX}\toprule
-          \emph{Frequency} & \emph{Bitrate} (Kbit/s) -- quality 0$\rightarrow$7 \\\midrule
-          44100Hz stereo        & 75, 80, 90, 100, 120, 140, 160, 170 \\
-          22050Hz stereo        & 39, 41, 45, 50,  60,  80,  110, 130 \\
-          44100Hz mono          & 65, 68, 73, 80,  90,  105, 125, 140 \\
-          22050Hz mono          & 35, 38, 40, 45,  50,  60,  75,  90 \\\bottomrule
-        \end{tabularx}
-      \end{center}
-    \end{table}
-  }
-  
-  \begin{description}
-  \item[Frequency:]
-    Choose the recording frequency (sample rate) -- 48kHz, 44.1kHz, 32kHz and
-    24kHz, 22.05kHz, 16kHz are available. Higher sample rates use up more disk
-    space, but give better sound quality.
-    This setting determines which frequency range can accurately be reproduced
-    during playback, Lower frequencies produce smaller files.
-    \opt{MASCODEC}{
-     The frequency setting also determines which version of the MPEG standard 
-     the sound is recorded using:\\
-     MPEG v1 for 48, 44.1 and 32\\
-     MPEG v2 for 24, 22.05 and 16\\
-    }
-    
-  \item[Source:]
-    Choose the source of the recording. This can be 
-    \opt{recorder,recorderv2fm,h1xx}{SPDIF (digital),} microphone or line in.
-    \opt{CONFIG_TUNER}{For recording from the radio see page \pageref{ref:FMradio}.}
-    
-    \opt{recorder,recorderv2fm,h100}
-        {\note{You cannot change the sample rate for digital recordings.}}
-    
-  \item[Channels:]
-    This allows you to select mono or stereo recording. Please note that 
-    for mono recording, only the left channel is recorded.  Mono recordings
-    are usually somewhat smaller than stereo.
-    
-  \item[Independent Frames:]
-    The independent frames option tells the \dap\ to encode with the bit
-    reservoir disabled, so the frames are independent of each other. This
-    makes a file easier to edit.
-    
-  \item[Time Split:]
-    This option is useful when timing recordings. If set to active it stops 
-    a recording at a given interval and then starts recording again with a 
-    new file, which is useful for long term recordings.
-    \newline
-    The splits are seamless (frame accurate), no audio is lost at the split 
-    point. The break between recordings is only the time required to stop
-    and restart the recording, on the order of 2 -- 4 seconds.
-    \newline
-    Options (hours:minutes between splits): off, 24:00, 18:00, 12:00, 10:00, 
-    8:00, 6:00, 4:00, 2:00, 1:20 (80 minute CD), 1:14 (74 minute  CD), 1:00, 
-    00:30, 00:15, 00:10, 00:05.
-    
-  \item[Prerecord Time:]
-    This setting buffers a small amount of audio so that when the record button 
-    is pressed, the recording will begin from that number of seconds earlier.
-    This is useful for ensuring that a recording begins before a cue that is
-    being waited for.\\
-    Options: Off, 1 -- 30 seconds
-    
-  \item[Directory:]
-    Allows changing the location where the recorded files are saved. The
-    default location is \fname{/recordings}.
-    
-  \item[Show recording screen on startup:]
-    If set to yes, the \dap\ will start up with the while recording screen 
-    showing.\\
-    Options: Yes, No\\
-    
-  \item[Clipping Light:]
-    Causes the backlight to flash on when clipping has been detected.\\
-    Options: Off, Remote unit only, Main and remote unit, Main unit only.
-    
-  \end{description}
-}
- 
 \section{\label{ref:playlistoptions}Playlist Options}
   This menu allows you to work with playlists. Playlists can either be created
 automatically by playing a file in a directory directly, which will cause all 
@@ -473,7 +196,7 @@ battery status, hard disk size and the amount of free space on the disk.
   for more details.
 }
 
-\opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD,IPOD_4G_PAD,IAUDIO_X5_PAD,IPOD_VIDEO_PAD}
+\opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD,IPOD_4G_PAD,IAUDIO_X5_PAD}
 {
 \section{Quick Menu}
   Whilst not strictly part of the \setting{Main Menu}, it is worth noting that a few
@@ -487,4 +210,3 @@ battery status, hard disk size and the amount of free space on the disk.
   (Page \pageref{ref:PlaybackOptions})
   and the \setting{Show Files} option (Page \pageref{ref:ShowFiles}).
 }
-
-- 
cgit v1.2.3

