From a507bb283782ee3adb1fc9ba0c6f094108ef558c Mon Sep 17 00:00:00 2001
From: Sebastian Leonhardt <sebastian.leonhardt@web.de>
Date: Mon, 20 Jul 2015 01:50:26 +0200
Subject: YH8xx,YH9xx: Keymap improvement

The main "innovation" in this patch are two "virtual buttons"
for the record switch on YH92x targets. When the switch state
changes, a single BUTTON_REC_SW_ON or .._OFF button event will
be generated. Thus keymap code can react on switching, but
not on the actual state of the switch.

Wherever sensible, the following user scheme is applied:
- use PLAY as confirm button
- use REW button or Long REW to exit
- use REC (YH820) or FFWD (YH92X) as modifier key for button combos

Change-Id: Ic8d1db9cc6869daed8dda98990dfdf7f6fd5d5a1
---
 manual/plugins/calculator.tex | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

(limited to 'manual/plugins/calculator.tex')

diff --git a/manual/plugins/calculator.tex b/manual/plugins/calculator.tex
index dd011c0ddc..c760ab1937 100644
--- a/manual/plugins/calculator.tex
+++ b/manual/plugins/calculator.tex
@@ -55,9 +55,10 @@ standard calculator. Pressing the ``1st'' and ``2nd'' buttons will toggle betwee
         & Delete last entered digit or clear after calculation\\
         %
     }
-    \opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD}{
+    \opt{RECORDER_PAD,IRIVER_H100_PAD,IRIVER_H300_PAD,SAMSUNG_YH820_PAD}{
         \opt{RECORDER_PAD}{\ButtonFTwo}
         \opt{IRIVER_H100_PAD,IRIVER_H300_PAD}{\ButtonMode}
+        \opt{SAMSUNG_YH820_PAD}{\ButtonRec}
        \opt{HAVEREMOTEKEYMAP}{& }
         & Cycle through the 4 basic operators\\
         %
@@ -81,7 +82,8 @@ standard calculator. Pressing the ``1st'' and ``2nd'' buttons will toggle betwee
         ,MROBE100_PAD,COWON_D2_PAD}{\ButtonPower}
     \opt{SANSA_FUZE_PAD}{Long \ButtonHome}
     \opt{GIGABEAT_S_PAD}{\ButtonBack}
-    \opt{PBELL_VIBE500_PAD,SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{\ButtonRec}
+    \opt{PBELL_VIBE500_PAD}{\ButtonRec}
+    \opt{SAMSUNG_YH92X_PAD,SAMSUNG_YH820_PAD}{Long \ButtonRew}
     \opt{MPIO_HD200_PAD}{\ButtonRec + \ButtonPlay}
     \opt{MPIO_HD300_PAD}{Long \ButtonMenu}
     \opt{SANSA_FUZEPLUS_PAD}{Long \ButtonBack}
-- 
cgit v1.2.3

