From 45c40b4231e67866887b6d6d740f1a3c3ba321a1 Mon Sep 17 00:00:00 2001
From: Michael DiFebbo <medifebbo@rockbox.org>
Date: Sun, 30 Jul 2006 13:40:17 +0000
Subject: Added textual player descriptions for blinds users for ipod video,
 ipod mini, ipod color, ipod 4g and h300.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@10367 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 90 ++++++++++++++++++++++++++++++---------
 1 file changed, 71 insertions(+), 19 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 01c11b98b4..69ec55d48d 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -14,41 +14,93 @@ Throughout this manual, the buttons on the \dap\ are labelled according to the
 picture above.
 
 \subsection{The \daps{} controls}
+
 \blind{
-  \opt{h1xx}{
-  If you lie the \dap\ on the table with the joystick pointing towards you, and
-  the curved sides at the top, the you will find the following if you start from
-  the top-right corner and follow the side of the \dap: \ButtonOn, \ButtonOff,
-  \ButtonMode, USB port, a small hole for resetting the \dap, charger plug,
-  \ButtonRec, headphone minijack plug, remote port, optical/line in,
-  optical/line out. The joystick in the middle of the \dap\ is used to navigate
-  menus by pressing it up/down and left/right. Pressing the joystick down is
-  labelled \ButtonSelect\ throughout this manual.
+
+  \opt{h1xx}{ 
+  If you lay the \dap\ on the table with the joystick pointing 
+  towards you, and the curved sides at the top, you will find the following 
+  if you start from the top-right corner and follow the side of the \dap: 
+  \ButtonOn, \ButtonOff, \ButtonMode, USB port, a small hole for resetting the 
+  \dap, charger plug, \ButtonRec, headphone minijack plug, remote port, 
+  optical/line in, optical/line out. The joystick in the middle of the \dap\ is 
+  used to navigate menus by pressing it up, down, left and right. Pressing the 
+  joystick down is labelled \ButtonSelect\ throughout this manual. }
+  
+  \opt{h300}{
+  Hold the lay the \dap\ so that the side with the button pad and 
+  LCD is facing towards you.  The buttons on the button pad are as follows:  top 
+  left corner: \ButtonOn, bottom left corner: \ButtonOff, top right corner: 
+  \ButtonRec, bottom right corner: \ButtonMode.  In the center of the button pad 
+  is a button labelled \ButtonSelect.  Surrounding the \ButtonSelect\ button are 
+  four directional buttons used to navigate up, down, left and right.
+  
+  On the top panel of the \dap, from left to right, you can find the 
+  following: headphone minijack plug, remote port, Line-in, Line-out. 
+  
+  On the bottom panel of the \dap, from left to right, you can find the 
+  following:  power jack and two USB ports.  The USB port on the right is used 
+  to connect your \dap\ to your computer.  The USB port on the left is not 
+  used in Rockbox. 
   }
+
+	\opt{ipod4g,ipodcolor,ipodvideo,ipodmini}
+	{ 
+	The main controls on the \dap\ are a slightly indented scroll wheel 
+	with a flat round button in the center. Hold the \dap\ with these controls 
+	facing you. 
+	
+	The top of the player will have the following, from left to 
+	right:
+		\opt{ipod4g,ipodcolor}{remote connector, headphone jack, hold switch.}
+		\opt{ipodvideo}{hold switch, headphone jack.}
+		\opt{ipodmini}{hold switch, remote connector, headphone jack.}	
+	
+  The dock connector that is used to connect your \dap\ to your computer is on 
+  the bottom panel of the \dap.
+
+  The button in the middle of the wheel is called \ButtonSelect. You can
+  operate the wheel by pressing the top, bottom, left or right sections,
+  or by sliding your finger around it.  The top is \ButtonMenu, the bottom is
+  \ButtonPlay, the left is \ButtonLeft, and the right is \ButtonRight.
+  When the manual says to \ButtonScrollFwd, it means to slide your finger
+  clockwise around the wheel. \ButtonScrollBack\ means to slide your finger
+  counterclockwise. Note that the wheel is sensitive, so you will need to move
+  slowly at first and get a feel for how it works.
+  
+  Note that when the hold switch is pushed toward the center of the \dap, 
+  ``hold'' is on, and none of the other controls do anything.  Be sure ``hold'' 
+  is off before trying to use your player. 
+
+  }
+	
   \opt{ipodnano}{
-  The main controls on the \playername{} are a slightly indented wheel with a
-  flat round button in the center. Hold the \dap{} with these controls on the
+  The main controls on the \dap\ are a slightly indented wheel with a
+  flat round button in the center. Hold the \dap\ with these controls on the
   top surface. There is a Hold switch at one end, and headphone and USB jacks
   at the other; be sure the end with the switch is facing away from you.
 
-  The button in the middle of the wheel is called \ButtonSelect{}. You can
+  The button in the middle of the wheel is called \ButtonSelect\. You can
   operate the wheel by pressing the top, bottom, left or right sections,
-  or by sliding your finger around it.  The top is \ButtonMenu{}, the bottom is
-  \ButtonPlay{}, the left is \ButtonLeft{}, and the right is \ButtonRight{}.
-  When the manual says to \ButtonScrollFwd{}, it means to slide your finger
-  clockwise around the wheel. \ButtonScrollBack{} means to slide your finger
-  counterclockwise. Note that the wheel is sensitive, so you'll need to move
+  or by sliding your finger around it.  The top is \ButtonMenu\, the bottom is
+  \ButtonPlay\, the left is \ButtonLeft\, and the right is \ButtonRight\.
+  When the manual says to \ButtonScrollFwd\, it means to slide your finger
+  clockwise around the wheel. \ButtonScrollBack\ means to slide your finger
+  counterclockwise. Note that the wheel is sensitive, so you will need to move
   slowly at first and get a feel for how it works.
 
-  Note that when the Hold switch is pushed toward the center of the \dap{},
+  Note that when the Hold switch is pushed toward the center of the \dap\,
   Hold is on, and none of the other controls do anything; be sure Hold is
   off before trying to use your player.
   }
-  \nopt{h1xx,ipodnano}{
+  
+  \nopt{h1xx,h300,ipodnano,ipodvideo,ipodmini,ipod4g,ipodcolor}
+  {
     \fixme{Write a section describing the \dap\ for blind users.}
   }
 }
 
+\subsection{Turning the \dap\ on and off}
 To turn on and shut down your \dap, the following keys are used:
 
 \begin{table}
-- 
cgit v1.2.3

